SN# DCEJ81172 and below get “D” version software Nov 2008 and up get “E” version 4th letter = month, 1st number is year

A Jan

B Feb

C Mar

D Apr

E May

F June

G July

H Aug

I Sept.

J Oct

K Nov

L Dec

1.       Determine the firmware version needed based on the color of the SD card reader, either 1.36 for the red SD card reader or 1.39 for the Dark Blue/Black SD card reader.

2.       Determine what mainboard the system has, either "D" or "E".

* + Consoles running firmware 1.01 thru 1.17a would be “D”
	+ Console running firmware 1.18 would be “E”

If running a newer firmware the unit serial number would be used.

* + For unit serials #DCE\_10001 thru #DCE\_81172, would use “D”.
	+ For serial #DCE\_81173 and all numbers after this, would use “E”

3.       Determine the jumper settings based on the type of hard drive or adapter and the type of SD card reader.

·         With Zip drive or Red card reader - set drive or adapter to MASTER

·         With Dark Blue/Black SD card reader - set drive or adapter to SLAVE

So for example, if you had a unit with serial number DCEL142405 and a black card reader, you would use firmware 1.39E and set the hard drive jumper to slave.