For now all Modular IP, PTP and IP input output cards need to be done.

Telnet to the frame's IP

Type: consoleMenu

Select 5 Vid 16x8 IO (select 6 for Mod 8x4 IO, select 4 for PTP Mezz)

Select 1 16x8 IO IP1 Take about 30min per board. Each IP board need to done (then select the next location. On fully loaded frame IO’s 1 thru 8 )

When you see SET TO RUN FROM Wait\_RUN\_AFTER\_RESET, BOARD 154 SLOT 9 (below in RED) you can upgrade the other IP board or If all boards are complete then power cycle the frame

select U upgrade ARM SW

Select 4 for the PTP card Select U upgrade ARM SW

Select 6 modular IO select U upgrade ARM SW (do each card)

Monitor the Web GUI for the frame (hit current button to refresh)

