TELNET TO THE FRAME FROM THE TOUCHSCREEN MENU PANEL

open a command prompt on the menu PC then type 
telnet 192.168.0.170 or whatever IP subnet you’re using (Frame IP)
at prompt type 
consoleMenu  (one word cap M only) 
select
(9) Debug
select
(15) Flash HADs
select
(M) Multi Boot Configuraton Image
select
Y for yes
start timer – (wait 10min)
The screen will display and error (unable to find a file) ignorne this 
you will not see anything occurring on screen so just wait it out
reboot the frame after 10min
keep an eye on the menu for HAD errors it is possible that they may need reflashed again although I have never seen it fail