It you have upgraded to V14.0 and the IS HAD are reporting out of date even after you’ve done the HAD update procedure to this:
 
Telnet to the frame.  
Enter the consoleMenu (case sensitive)
Enter 7 (for Image Store)
Enter 10 (for HAD)
Enter 7 (for Program_FLASH)
Enter g (for Golden Configuration Image
Enter b/3 (the correct version/revision)
Enter w (for write)
Enter y (to confirm)
Wait for it to finish, a couple of minutes. 
Power cycle the frame. 
 
It will look like the text below when you actually do it.

-> consoleMenu
[1] Status                [2] Controller            [3] ME
[4] Input                 [5] Output                [6] ModIO
[7] Image Store           [8] Spare                 [9] Debug
[10] Software Options     [11] Fan Controller       [P] Power Supply
[H] Boot Sw Help          [Z] Test Diagnostics      [D] DisableAllUpdates
[M] DisableAllMonitoring  [x] Exit to shell
> 7
[1] Peek                  [2] Poke                  [3] BlockPeek
[4] LongPeek              [5] LongPoke              [6] LongBlockPeek
[7] Image Store DPM       [8] IP Config             [9] Image Store Features
[10] HAD                  [B] Board ID              [T] Temp Monitor
[D] DisableBoardUpdates   [x] Exit
Image Store> 10
[1] Peek                  [2] Poke                  [3] BlockPeek
[4] LongPeek              [5] LongPoke              [6] LongBlockPeek
[7] Program_FLASH         [V] Show Version Info     [x] Exit
HAD> 7
Select FLASH Type
[G] Golden Configuration Image
[M] Multi Boot Configuration Image
[x] Exit (At any time, 'x' will exit)
> g
Specify Version/Revision or Filename?
        For Version/Revision: <Version>/<Revision> [e.g. a/0 or b/1...]
        For Filename: -name <filename> [e.g. -name test_had.000]:
> b/3
Read or Write?
[R] Read               [W] Write
> w
Summary:
        Flash Type:     Golden
        RBF File:       /ahci00:2/boot1/FPGA/enc_ishad_golden_b.003
        R/W:            w
Is this correct? (Y or N)> y
HAD E1800000: ImageStore 2, Num.Ver.Rev 5000.b.3, TimeStamp 05/14/2018 11:06, DMA:N/A
HAD E1800A00: Flashing file "/ahci00:2/boot1/FPGA/enc_ishad_golden_b.003" with 1488064 bytes at flash offset 0x000000 (t
ry 1)
HAD E1800A00: Erase sector 0000, dest addr 0x000000 (00%)
HAD E1800A00: Erase sector 0001, dest addr 0x010000 (04%)
snip
HAD E1800A00: Erase sector 0021, dest addr 0x150000 (91%)
HAD E1800A00: Erase sector 0022, dest addr 0x160000 (95%)
HAD E1800A00: Program page 0000, dest addr 0x000000 (00%)
HAD E1800A00: Program page 0100, dest addr 0x006400 (01%)
snip
HAD E1800A00: Program page 5800, dest addr 0x16a800 (99%)
HAD E1800A00: Flashed successfully (tries 1)!
[1] Peek                  [2] Poke                  [3] BlockPeek
[4] LongPeek              [5] LongPoke              [6] LongBlockPeek
[7] Program_FLASH         [V] Show Version Info     [x] Exit
HAD>