1) Press the key of [Ctrl]+[Alt]+[F5] at the same timing on the USB keyboard

(2) Please enter "jig" as Login Name and "jig" for Password on the USB keyboard

(3) Please enter "ping 10.129.2.1" on the USB keyboard

(4) Please let us know the information displayed on the menu panel.