MVS-3000-65xx Install

Save all switcher Setup, User, snapshot, effects to USB.
Download software from ftp://systems:sony@65.196.27.198  Product Software/MVS65XX 3000/MVS-65xx_3000v1.01zip, extract contents of zip to root directory of USB thumb drive.
Go to Menu 7316, press Install, select Device: UI in upper window.  User interface software on USB is auto listed in lower window, press Set (denoted w/a check on rh side).  Select Device: Pnl1, press Set.  Select Device: Swr1, select file below MVS-3000 Proc (Full), Execute.  When it’s done select Device: Swr1, file MVS3000-FPGA [v1.01] for Upgrade install, Set, Execute to install this last component separately.  If any software doesn’t completely install, DO NOT power off the switcher.
Once software is updated successfully, bit 4 reset must be executed.  Execute organized switcher shutdown: press Page/Shutdown, power MVS main frame off when menu screen goes black.  Remove CA-85 bd, switches S1302 location J-1 and S3802 location D-1, turn bit 4 ON for both.  Insert bd, power up, a countdown is displayed on 7 segment display; wait for two dashes to appear appox 30 seconds or less.  Power off MVS frame, remove CA-85, and restore switches to OFF position.
Power up MVS mainframe, wait for it to boot.  Menu 7313 change Ref Input Format from Tri-level to BB, select proper Signal Format.  Menu 7311, Auto Config, Yes then Define.   Menu 7314, select Start Up Mode: Custom, Setup: User, Init Status: User then Execute.  Check versions Menu 7316
Load setup file, to save to NVRAM Menu 7314, Setup Define, Init Status Define for Swr1 and Pnl1 each separately