DirectOut ANDIAMO / ANDIAMO 2 Firmware ReadMe, 2018-05-22

Version 6.7
- MADI receiver: unlock detection improved

Version 6.6
- new feature: Front panel brightness dimmable
- improved mute behaviour during start-up

Version 6.4
- new feature: summing bus with dithering
- improved behavior of DA-Mutes

Version 6.1:
- phase reverse issue at analog output (only devices with new DA converters) <= fixed

Version 5.3
- fix in gui

Version 5.1
- fixed issue with AES at 4 FS (XT only)

Version 4.9:
Features:
- Output Gain for analog outputs
- 'Mute All' Function for output gains
- AD/DA Calibration - adaption of AD/DA reference level in 0.1 dB steps. The calibration is applied when the ANDIAMO is set to input or output level 'LOW'.
- 4 FS Support - sample rates up to 176,4 / 192 kHz
- Disable MADI remote - New switch, forces remote functionality to USB only, even if there is incoming control data via MADI.

The new features are accessible with ANDIAMO Remote v2.5 or higher.

Version 4.1:
Features:
- 'Display Dark' added to mute LED display
- 'Identify' added to determine selected device (in scenarios with several devices involved)
- 'Extended Routing' added for devices with two MADI ports => individual access control of the two MADI I/Os

Version 3.4:
Bugfix:
- Userbit transparency for AES I/Os was turned on by default preventing Serial-over-MADI from working <- fixed

Version 3.3:
Bugfix:
- SRC settings were not restored correctly after reboot (ANDIAMO.XT SRC and ANDIAMO 2.XT SRC only)

Version 3.2:
Features:
- supports DARS (AES11) as sync source for WCK input

Version 3.1:
Features (ANDIAMO 2 only):
- Priority setting for redundancy mode -> switch-back to priority port if signal returns (setup requires Software v1.4.1)

Version 3.0
Bugfixes:
- Delay compensation did not work since last firmware release <- fixed

Version 2.9
Features:
- redundancy mode switchable (ANDIAMO 2 only)

Version 2.8
- Maintenance update (one Firmware release number for the complete ANDIAMO Series)

Version 2.5
- Improved stability of serial embedder

Version 2.4
Features:
- Remote Control support
- Matrix Mode:
  NOTE: The Matrix Mode can be activated and de-activated without software on the front panel:
	Select the Bank menu, press and hold the SET button until both Bank LEDs are lit (Matrix Mode on)
	The same procedure de-activates the Matrix Mode and returns to standard Bank routing.
	The current Matrix routing is stored in the background and can be used without software connection at any time.

- Fan Control via Software

Version 1.8
Features:
- MADI Input no lock -> Out Level blinks slowly

- Delay Compensation:
If ANDIAMO sees an ANDIAMO at its MADI input, delay compensation for the MADI output is applied.
Active delay compensation is dipslayed by 'heart beat' on bank LED.

Bugfixes:
- Channel 56 not available on 56ch MADI input <- fixed

DirectOut GmbH, 2014