@echo off
prompt $p$g
path C:\;C:\DOS;C:\UTILS
doskey

REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
REM !!DON'T REMOVE THE FOLLOWING LINES               !!
REM !!                                               !!
REM !!CURRENT_OS_TYPE=WCE                            !!
REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
REM !!                                               !!
REM !! MAKE SURE YOU SET THE RIGHT IRQ & IOBASE      !!
REM !! FOR YOUR NETCARD BELOW.                       !!
REM !!                                               !!
REM !! NET_IRQ can be specified in either hex or     !!
REM !! decimal digits (ie either as IRQ=E or IRQ=14).!!
REM !! A value of 0 for both NET_IRQ & NET_IOBASE    !!
REM !! requests that the first network card found on !!
REM !! the PCI bus should be used.                   !!
REM !!                                               !!
REM !! NET_IOBASE must be specified in Hex digits.   !!
REM !! A value of 0 for NET_IOBASE means to auto     !!
REM !! searchfor the PCI net card using the          !!
REM !! specified IRQ value.                          !!
REM !!                                               !!
REM !! NET_IP can be set to specify a static IP      !!
REM !! address or left blank to use DHCP to obtain   !!
REM !! an IP address.  Format of set should be:      !!
REM !!      set NET_IP=10.0.0.1                      !!
REM !!                                               !!
REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
set NET_IRQ=0
set NET_IOBASE=0
set NET_IP=0.0.0.0
set NET_MASK=255.255.255.0
set NET_GATEWAY=0.0.0.0
set HOSTNAME=Ce_XXX_NNN

REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
REM !! For VGAMODE you can use the following values  !!
REM !! set VGAMODE=VGA                               !!
REM !! set VGAMODE=PAL                               !!
REM !! set VGAMODE=NTSC                              !!
REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
set VGAMODE=VGA
REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
REM !! For KBDLAYOUT you can use the following values!!
REM !! Layout US :                                   !!
REM !! set KBDLAYOUT=409                             !!
REM !! Layout FRENCH :                               !!
REM !! set KBDLAYOUT=40C                             !!
REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
set KBDLAYOUT=409

if EXIST c:\cecfg.bat call c:\cecfg.bat
if EXIST c:\lsmce\data\evs\vgacfg.bat call c:\lsmce\data\evs\vgacfg.bat

REM !!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
REM !! if a version > than 9.0 has been installed,   !!
REM !! the file c:\lsmce\code\cesnmp.dll exist but   !!
REM !! must not be loaded in V9                      !!
if EXIST c:\lsmce\code\cesnmp.dll del c:\lsmce\code\cesnmp.dll



set MENUOPTIONS=/t
set VGA2TVEXE=vga2tv_N.exe

vgaregs c:\lsmce\os\vgaregs.bin

echo.
echo PRESS [ALT]+[BACKSPACE] TO TOGGLE BETWEEN VGA AND VIDEO MODES.
echo.
seconds 3

:VGA2TV
cd c:\utils
del hardwcfg.bin
copy c:\lsmce\data\hardwcfg.bin
if %VGAMODE% == NTSC goto NTSC
if %VGAMODE% == PAL goto PAL

:VGA
echo /T > vga.opt
%VGA2TVEXE% < vga.opt
del vga.opt
goto MENU

:PAL
%VGA2TVEXE%
goto MENU

:NTSC
echo /N > vga.opt
%VGA2TVEXE% < vga.opt
del vga.opt
goto MENU


:MENU
cd c:\utils
set MENULOOP=0
menu.exe %MENUOPTIONS%
set MENUOPTIONS=
call menu.bat
if %MENULOOP% == 1 goto MENU
