General features

* Tally configuration files now reside on TSI-4000, not on the local PC.
* Source name changes and UMD overrides are now synchronized between Tally Console and Web Console
* Ability to quickly switch configurations within TSI-4000 without re-upload from tally console. This switch can executed from Web Console or Tally Console
* TSI-4000 maintenance console now included in Web Console for convenient system upgrades and diagnostics.
* Web console is multi-user with admin-controlled user access to system features

New device interfaces

* Calrec audio panel control
* Ross Ultrix router interface
* Receive of Image Video protocol
* ATEM switcher interface
* OES scoreboard interface
* Daktronics scoreboard interface
* Shotoku camera interface (over TSL5)