**LV5800: SOFTWARE RELEASE NOTES**

**To view the software version, press these keys in the following order: [SYS] 🡪 [F5] SYSTEM INFORMATION.**

| **UPDATE** | **NOTES** |
| --- | --- |
| Version 11.2 | Improvements:* Bug fixed for Japanese Closed Captions.
 |
| Version 11.0 | Improvements:* Bug fixed for Japanese Closed Captions.
 |
| Version 10.6 | New Function:* Frame Marker function.

Improvements:* Added Aspect Ration markers for 14:9, 13:9, and 2.39:1.
* Added decimal scale for 8 bits and 10 bits on the WAVEFORM display.
 |
| Version 9.6 | New Functions:* Loudness measurements.

Improvement:* Mute signal detection for LV5800-OP40A (Digital Audio & Analog Audio).
 |
| Version 9.0 | New Function:* Tri-level Sync Composite (LV5800-OP03A) capabilities.
 |
| Version 7.0 | New Function:* Lip Sync capabilities for SD-SDI and HD-SDI signals.

Improvement:* Added Y/R/G/B display on the Histogram mode.
 |
| Version 6.8 | New Function:* Added the CIE chart (BT.709) for HD.

Improvement:* Added the Loudness graphic log display on LV5800-OP40A (Digital Audio & Analog Audio).
 |
| Version 4.8 | New Functions:* SNTP Support is added and it can display the time and date from a time server.
 |

| **UPDATE** | **NOTES** |
| --- | --- |
| Version 4.7 | Improvements:* Improvements have been made so that the screen capture data can be saved in to a USB memory device with two actions. File names are now automatically generated combining date and time information.
 |
| Version 3.7 | New Function:* Beeper sound is activated if an error is detected.
 |
| Version 3.4 | New Functions:* Single input mode is added.
* Input unit can be remotely controlled via the remote connector on the rear panel.
 |
| Version 3.1 | Improvement:* Window frame color can be changed.
 |
| Version 1.6 | New Functions:* Frame Capture function is added.
* Current Color System can be displayed in the WFM display mode.
* ON/OFF Display function is added for TIME, INPUT INFORMATION, etc.
* Frame can be erased in the single screen mode.
* PLATFORM tab menu is added to the SYSTEM menu.

Improvement:* MULTI menu is moved to the SYSTEM menu.
 |