**LV5800: SOFTWARE RELEASE NOTES**

**To view the software version, press these keys in the following order: [SYS] 🡪 [F5] SYSTEM INFORMATION.**

| **UPDATE** | **NOTES** |
| --- | --- |
| Version 11.2 | Improvements:   * Bug fixed for Japanese Closed Captions. |
| Version 11.0 | Improvements:   * Bug fixed for Japanese Closed Captions. |
| Version 10.6 | New Function:   * Frame Marker function.   Improvements:   * Added Aspect Ration markers for 14:9, 13:9, and 2.39:1. * Added decimal scale for 8 bits and 10 bits on the WAVEFORM display. |
| Version 9.6 | New Functions:   * Loudness measurements.   Improvement:   * Mute signal detection for LV5800-OP40A (Digital Audio & Analog Audio). |
| Version 9.0 | New Function:   * Tri-level Sync Composite (LV5800-OP03A) capabilities. |
| Version 7.0 | New Function:   * Lip Sync capabilities for SD-SDI and HD-SDI signals.   Improvement:   * Added Y/R/G/B display on the Histogram mode. |
| Version 6.8 | New Function:   * Added the CIE chart (BT.709) for HD.   Improvement:   * Added the Loudness graphic log display on LV5800-OP40A (Digital Audio & Analog Audio). |
| Version 4.8 | New Functions:   * SNTP Support is added and it can display the time and date from a time server. |

| **UPDATE** | **NOTES** |
| --- | --- |
| Version 4.7 | Improvements:   * Improvements have been made so that the screen capture data can be saved in to a USB memory device with two actions. File names are now automatically generated combining date and time information. |
| Version 3.7 | New Function:   * Beeper sound is activated if an error is detected. |
| Version 3.4 | New Functions:   * Single input mode is added. * Input unit can be remotely controlled via the remote connector on the rear panel. |
| Version 3.1 | Improvement:   * Window frame color can be changed. |
| Version 1.6 | New Functions:   * Frame Capture function is added. * Current Color System can be displayed in the WFM display mode. * ON/OFF Display function is added for TIME, INPUT INFORMATION, etc. * Frame can be erased in the single screen mode. * PLATFORM tab menu is added to the SYSTEM menu.   Improvement:   * MULTI menu is moved to the SYSTEM menu. |