Programming
 Instructions
For Programming most KENWOOD 2-WAY Radios
 you will need the following equipment:

1.	An IBM compatible computer running DOS (Recommend DOS 6.22) for programs thru KPG-49D
2.	Newer programs KPG-52D and Later releases, require Windows 98 or newer. I use XP.  I’m also able to open and use the MSDOS programs with Windows 98SE and XP OS.

3.	A KENWOOD COMPATIBLE RADIO PROGRAMMING CABLE - (Kenwood does not use a Rib Box, the electronics are built into the cable.) Schematics are included on this cd. Or you can purchase some cables through other Ebay members like;
Ed
http://cgi6.ebay.com/ws/eBayISAPI.dll?ViewSellersOtherItems&userid=ed2wayprogramming
Panter
http://cgi6.ebay.com/ws/eBayISAPI.dll?ViewSellersOtherItems&userid=panter88&completed=0&sort=3&since=-1
Radioprogramming
http://cgi6.ebay.com/ws/eBayISAPI.dll?ViewSellersOtherItems&userid=radioprogramming&completed=0&sort=3&since=-1

3. The Specific Radio Software that covers your radio.  
    SEE THE SOFTWARE REFERENCE GUIDE BELOW

4. If the KPG software, that you are installing, requires a Registration number Please open the document on this CD named Kenwood Software. I’ve also included the software list below, on this document. Scroll down to the KPG that you’re installing, look to the right, below the list of radios programmed, you’ll see the reg id.
5. Some software, can be installed off the CD. Most Older software, needs to be copied or (Un zipped) onto your Hard Drive (C:\) into a directory like Kenwood.

COMPUTERS

1.As far as operating systems go you will want to use just plain old DOS. Most Kenwood software is designed to run in DOS (Except for the Windows Based Programs)
DO NOT USE WINDOWS OR DOS BASED WINDOWS FOR THE DOS BASED PROGRAMS, YOU WILL HAVE TO BOOT UP TO TRUE DOS.
2. If you don’t currently have DOS 6.22 you need it, a DOS 6.22 boot disk is included on this CD (More info on DOS is located on the last page) I However, do NOT RECOMMEND using a Boot Disk.

3. The specific Radio Service Software that covers your radio.  
    SEE THE SOFTWARE REFERENCE GUIDE BELOW
   WOOD PROGRAM
 MING INSTRUCTIONS
PROGRAMMING STEPS

1.	Boot your computer in DOS, for the programs that Require MSDOS Which means, turn on Computer, and it shows( C:\ ) (NO WINDOWS)
2.	Boot up your computer into Windows 98SE, Windows 2000, Windows XP Now you’re ready to use, Install KPG programs designed for Windows OS.
3.	Attach the programming cable to the Com Port and Radio.
4.	Turn the radio on and out of scan mode. (Some models of Kenwood require the radio to be put into program mode by holding down 2 or more buttons on the radio and then turning the radio on. The help file in the software will tell you what to do if this applies to your radio. (Newer Kenwood radios do not require this.)
5.	Attach the 9 volt battery to the programming if it has a 9 volt lead.
6.	Start the software. Boot up to DOS, the easiest way to do this is to have the Kenwood Software already on a floppy disk remove the DOS disk from your floppy and insert the Kenwood Software disk. (For example, at the A: prompt type kpg36d.exe. The software should start).
7.	 Read the radio (Be sure and try both Com Ports under settings, Com 1 and Com 2, to see which Com Port you have the cable programmed into)
8.	 Edit the radio data and program to radio.

TROUBLE??

1. Try both Com Ports from the setup menu within the software. 
Run in DOS!
2. Clean the radio and programmer pins with rubbing alcohol. 

DOS INFORMATION
Much of the older radio software must be run in DOS.

Included on this Programming CD is a DOS Boot Disk

1. Click on the program and open to a blank floppy in drive A:

2. When finished making the disk, restart the computer with the disk in drive A:

3. REMOVE THE DOS DISK

YOUR COMPUTER SHOULD NOW BE IN DOS

Place the radio programming disk in drive A: 
                     If  the A:  prompt appears simply type the name of the program, example kpg29d.exe

If the C: prompt appears type A: and hit the enter key.

Then type in the name of the program, example kpg29d.exe
The software will open.

Be sure and try both Com Ports in the Software.

KENWOOD 
        SOFTWARE/PROGRAMMER CROSS REFERENCE
KPG-5D	2.14	TK-930 / 931 UPDATED9/04	
KPG-6D	1.30	TK-705D / 805D TK-706D / 807D	
KPG-7D	2.01	TK-830 / 730 / 630	
KPG-9D	1.40	TK-240D / 340D	
KPG-11D	1.25	TK-230 / 330	
KPG-13D  UK	1.04		
KPG-15D	1.01	KDS-10  (TWO TONE DECODER)	
KPG-16D	1.10	TK-430 / 431	
KPG-20D	1.04	TK-709T / TK-349T	
KPG-21D	1.00	TKR-720 / 820 
TKB-620 / 720	
KPG-23D	1.01	TK-250 /350	
KPG-25D	3.00	TK-940 / 941 / 840/ 841	
KPG-26D	1.00	TK-353 LTR	
KPG-27D	5.00	TK-260 / 270 / 278 / 272 
TK-360 / 370 / 378 / 372 / 388	
KPG-28D	1.00	TK-759 / 859/ / 752 / 852	
KPG-29D	2.10	TK-760 / 762 / 768 TK-860 / 862 / 868	
KPG-32D	1.00	TK-259 / TK-359	
KPG-34D	2.00	TK-261 / TK-361	
KPG-34D_LAB	V.7-03	TK-261/ TK-361	
KPG-35D	1.00	TK-480 / 481	
KPG-38D	1.01	TK-290/390	
KPG-41D  UK	1.12	TK-715 \ TK-255	
KPG-44D	2.0	TK-690\TK-790\ TK–890	
KPG-44D	2.01	TK-690 / 790 / 890
RegNumber; 044K44410108AVIE	
KPG-47D	3.00	TKR 830/740/840  UPDATED 9/04
RegNumber; 047K44999999AWUA	
KPG-48D	1.00	TK-2100 / 3100 / 3101	
KPG-48D_LAB	V.7-03	TK-2100 / 3100 / 3101	
KPG-49D	2.00	TK-280 / 380  / 780 / 880 / 980 /981	
KPG49D_302	3.02	TK-280 / 380  / 480/ 481 /  780 / 880 / 980 /981	
KPG49D	4.01	TK-280 / 380  / 480/ 481 /  780 / 880 / 980 /981
RegNumber; 049K44490022AVIW	
KPG-52D	1.00	UBZ-LH14	
KPG-54D_LAB	1.00	TK-3101	
KPG-55D	2.01	TK-2102A / 2107A / 3102A / 3107A	
KPG-56D	2.00	TK-762G / 768G / 760G / 862G / 868G / 860G / 260G / 270G / 278G / 360G / 370G / 378G 	
KPG56D-V2.10	2.10	TK-260G / 360G  /  270G / 370G/ 272G/ 372G 
TK-760G / 762G / 860G / 862G
RegNumber: 056K44160112AVFZ 	
KPG56D-V300SCN	3.00	TK-260G / 360G  /  270G / 370G/ 272G/ 372G 
TK-760G / 762G / 860G / 862G
RegNumber: 056K44160258AVUF 	
KPG-56D- Version 4	4.00	TK-260G / 360G  /  270G / 370G/ 272G/ 372G 
TK-760G / 762G / 860G / 862G
RegNumber 056K44160112AVFZ	
KPG-56D	4.21	TK-260G / 360G  /  270G / 370G/ 272G/ 372G 
TK-760G / 762G / 860G / 862G
RegNumber 056K44160112AVFZ	
KPG-59D	2.10	TK-190 / TK-6110	
KPG-60D	1.01	RegNumber; 060K44999999AWTJ	
KPG-62D	1.00	TK-285 / 385  TK-785 / 885
RegNumber: 062K44230072AVHW	
KPG-65ED		Fleet Sync	
KPG-66D	 2.01	Repeater TKR750/850 KENWOOD
RegNumber:066K44999999AWUF	
KPG-66ND	1.00B16	Repeater TKR750/850 KENWOOD
RegNumber:066K44999999AWUF	
KPG-67D	1.00	TK-260G / 270G / 360G / 370G / 760G / 762G / 860G / 862G
RegNumber; 067K44999999AWUH	
KPG-69D	1.11	TK-2118 / 3118
RegNumber: 069K44999999AWUL	
KPG-70D	2.00	TK-7102\8102 MOBILE
RegNumber;070K44310008AVGX 	
KPG-70D	3.00	TK-7102 / TK-7108 / TK-8102 / TK8108
RegNumber;070K44310008AVGX	
KPG-71D	1.10	KDS-100 MDT / MESSAGE TERMINAL
RegNumber; 071K44190000AVEG	
KPG-71D	1.30	KDS-100 MDT / MESSAGE TERMINAL
RegNumber; 071K44190000AVEG	
KPG-73D	1.01	KGP 2A/2B
RegNumber; 073K44190000AVEK	
KPG-74D	1.10	TK-2140 & TK-3140 PORTABLES
RegNumber; 074K44410108AVIH	
KPG-74D	1.11	TK-2140 & TK-3140 PORTABLES
RegNumber; 074K44410108AVIH   9/04	
KPG-75D	1.10	TK-3130 & TK-3131 PORTABLES
RegNumber; 075K44999999AWUE	
KPG-76D	1.10	TK-373 LTR PORTABLE
RegNumber;076K44999999AWUG	
KPG-77D	1.00	TK-782  220MHz MOBILE
RegNumber; 077K44999999AWUI	
KPG-79D	1.01	TK-7150 & TK-8150 MOBILE
RegNumber; 079K44490022AVIZ	
KPG-80D	1.02	TK-7100 / TK-8100
RegNumber; 080K44310008AVGY	
KPG-82D	2.01	TK-2160 / TK-2168 / TK-3160
RegNumber;082K4456K287AWUD	
KPG-82D	2.02	TK-2160 / TK-2168 / TK-3160
RegNumber;082K4456K287AWUD	
KPG-82D	2.03	TK-2160 / TK-2168 / TK-3160
RegNumber;082K4456K287AWUD	
KPG-87D	1.00	TK-2202 / TK-2206 / TK-2207 / TK-3202 / TK-3206 / TK-3207 
RegNumber; 087K44999999AWUJ	
KPG-88D	1.00	TK-22002 / TK-32002 (Windows) 
 RegNumber 088K44999999AWUL	
KPG-89D	1.00	TK-7180/8180/2180/3180
RegNumber; 089K44999999AWUU	
KPG-89D	1.02	TK-7180/8180/2180/3180
RegNumber; 089K44999999AWUU	
KPG-89D	1.10	TK-7180/8180/2180/3180
RegNumber; 089K44999999AWUU	
KPG-91D	2.00	TKR-751  TKR-851
RegNumber; 091K44190000AVEI	
KPG-99D	1.01	TK-7160/8160
RegNumber; 099K4468K105AWIH	
KPG-100D		TK-2212 / 2217 / 3212 / 3217 (Windows) RegNumber100K53999999AWLZ	
Kpg-101D	1.01	TK-2170/3170/3173
RegNumber; 101K447BK121AWJZ	
KPG-118D	1.10	RegNumber: 118K4406K023AWDX	
KPG-118D	1.11	RegNumber; 118C4707Z12FAXIX