BPU4000 Version 4.50

Upgrade the software as necessary.

In case of upgrading, upgrade the peripheral units as necessary by referring to the related technical memos.

■Recommended software versions

・HDC4300 ：V1.80 or Higher

・HDC-P43 ：V1.80 or Higher

・HDCU2000/2500 ：V3.50 or Higher

・MSU-1000/1500, RCP-1500/1501/1530：V3.70 or Higher

・MSU-3000/3500 ：V1.21 or Higher

・RCP-3500,RCP3501 ：V1.20 or Higher

・RCP-3100 ：V1.00 or Higher

・HDCU3100 ：V2.80 or Higher

・HDCU3500 ：V1.80 or Higher

・F65 ：V4.01 or Higher

・PMW-F55 ：V9.20 or Higher

・CA4000 ：V2.51 or Higher

<Error Correction>

1. Fixed the symptom that white spots are displayed at the bottom of the screen when 720 HFR Format.

2. Fixed the communication problem when a network delay occurs. Fix a bug that the value displayed on the PANEL and the setting value actually reflected may differ when a network delay occurs and operating from MSU/RCP

**[Confirmation after Upgrading]**

|  |  |
| --- | --- |
| Confirm the versions in the CAMERA APP and each PLD item of the menu of BPU4000, SERVICE - <SOFTWARE PACKAGE> (S01) page and <PLD PACKAGE> (S02) page. CAMERA APP | V4.50 |
| OS | V1.03 |
| SY | V2.00 |
| DEC | V2.11 |
| DEC(F65) | V2.01 |
| DEC(F65 2X) | V2.10 |
| DEC(HDC4300) | V3.41 |
| DPR | V2.21 |
| DPR(HCO) | V2.00 |
| DPR(F65 2X) | V2.20 |
| DPR(SUB) | V1.10(\*1) |
| 4K-POST | V3.31 |
| 2K-POST | V3.30 |
| SDP | V3.22 |
| TX | V3.20 |