HDCU 2500 Version 3.50

<New Functions>

1. Functions have been added so that the HDCU2000 series can be used in combination with HDCE-TX30 and HDCE-RX30.

2. Added 2019 to the version of PAYLOAD ID.

Compliant with SMPTE ST292-1:2018, SMPTE ST372:2017, SMPTE ST425-1:2017, SMPTE ST425- 3:2019, and SMPTE ST425-5:2019.

<Error Correction>

1. Fixed an issue where Master devices could not be connected when CNS Mode was set to MCS.

**[Confirmation/Adjustment]**

<Confirming the software version>

Check the ROM version at the CHARACTER output or the MONITOR output.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

| \*ROM Version\* |

| CHU |

| CCU HDCU2000 |

| 3.50 21.xx.xx |

|\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_|