“Scan Interval” has been added to the “Panel” setting of the “Property”.

TOOL/PROPERTY/PANEL then select “SCAN INTERVAL” window at page bottom.

The command scanning interval of the system monitoring screen can be set within 2 to 8 seconds.

The larger the interval, the less load on the network using many cameras．

Please try to set it to 4 seconds．