**RCP1500 V 3.60**

**[Change Points]**

<New Functions>

1. Look setting for Return Video
2. HFR Detail Ratio setting screen is added in Paint menu
3. Gain Limit setting item is added on ARIA setting screen
4. Integrate Back Focus setting into Zoom/Focus setting screen, and add Zoom Tele End/Wide End button
5. Added a function that can be assigned to Custom SW

<Function Change / Function Improvement>

1. The optical condition bar display was changed to reflect not only the received light level but also the occurrence status of transmission failure.

* When there is a transmission failure that seems to be affected by the optical reflection at the optical fiber joint, "RX Reflection Warning/Care" is displayed at the top of the screen.

1. Changed the wording displayed at the top of the screen when the CCU light receive level drops

(Before) SDI Warning, SDI Care

(After) RX Level Warning, RX Level Care