DVS Switcher (V4.00乣) 巇條偺曗懌偲惂尷帠崁             Sep. 1, 2004
                                                  仮c1  Sep.27, 2004
                                                  仮c2  Oct.14, 2004
                                                  仮c3  Apr.08, 2005
                                                  仮c4  Jul.29, 2005
                                                  仮c5  Aug.04, 2005
                                                  仮c6  Jun.28, 2006
                                                  仮c7  Nov.30, 2006
                                                  仮c8  Jan.19, 2007
                                                  仮c9  Aug.16, 2007
                                                  仮c10 Nov.27, 2007
                                                  仮c11 Dec.19, 2007
                                                  仮c12 Jan.18, 2008
                                                  仮c13 Feb.22, 2008
                                                  仮c14 Mar.14, 2008
                                                  仮c15 Apr.01, 2008
                                                  仮c16 Apr.15, 2008
                                                  仮c17 Jul.16, 2008

    埲慜偺僶乕僕儑儞傑偱偵儕儕乕僗僲乕僩偵柧婰偟偨惂尷帠崁摍偵偮偄偰偼
    徣棯偝傟偰偄傞応崌偑偁傞丅

1. 儕僄儞僩儕惂尷

    丒System Format丄CCR Option丄Multi Format Option 偺桳柍丄偍傛傃
      Keep Window (乽Appendix-1 偺 (1)乿傪嶲徠) 偺 愝掕偵傛偭偰丄Key 慺嵽偵
      慖戰壜擻側儕僄儞僩儕偺忦審偑曄壔偡傞丅
      徻嵶偼乽Appendix-2. Key 慺嵽偺儕僄儞僩儕忦審偵偮偄偰乿傪嶲徠偡傞偙偲丅

1-A-1. Resume 摍偺婲摦帪偺儕僄儞僩儕    仮c15

  (1) Resume 摍偺婲摦帪丄儕僄儞僩儕偑暅尦偝傟側偄応崌偑偁傞丅
      - MP2 Reentry 偱壜擻偲側偭偨儕僄儞僩儕
      - Setup 偲偺慻傒崌傢偣偱丄晄壜偲側偭偨儕僄儞僩儕


2. Multi PGM Mode 偵娭偡傞惂尷

    丒Common 偲 Local 偺 Trans Type 楢摦摦嶌偵偮偄偰丅

      - Next Trans 偵 Bkgd 偲 Key 傪慖戰偟丄Trans Type 傪椉曽偲傕 Wipe 偵
        偟偨応崌丄僷僞乕儞傪摨偠偵偟偰傕僒僀僘摍偼堎側傞丅

      - 堎側傞僩儔儞僕僔儑儞僞僀僾乮摿偵 Wipe&DmeWipe乯偵傛傞摨帪僩儔儞僕僔儑儞
        偺幚峴偱偼丄偦傟偧傟偺棟榑揑側摦嶌僞僀儈儞僌偑堦抳偡傞偺傒偱丆
        搑拞偺夋偑堦抳偡傞偲偄偆傕偺偱偼側偄丅

    丒Pst Color Mix 偼 Next Trans 偑 Bkgd 偺応崌偺傒丄摦嶌傪曐徹偡傞丅

      - Trans Type 偵 Pst Color Mix 偑慖戰壜擻偲側傞偺偼丄Next Trans 偵 Bkgd
        偺傒丄Key1乣4 偑慡偰 Off 偺応崌偺傒偱偁傞丅
      - Pst Color Mix 拞偺 Next Trans 偵偍偄偰丄Bkgd 偲 Key 偺崿嵼傪嬛巭偡傞丅
      - Bkgd 偺 Trans Type 偑 Pst Color Mix 偺帪丄Local Trans 憖嶌傪嬛巭偡傞丅
        (Local Lever 偼 Non-sync 偲側傞丅)

    丒Pattern Limit 偼 Bkgd 偺 Trans Type 偑 Wipe丄偁傞偄偼 DME Wipe 偺帪偺傒
      偲偡傞丅

    丒DmeWipe 抶墑惂屼偺塭嬁    仮c4 捛壛

        Next Transition 偵 Bkgd 偲 Key 傪乮暪偣偰乯慖戰偟丄
        TransType 偑 DmeWipe 偲偦傟埲奜偺応崌丄僞僀儈儞僌傪崌傢偣傞偨傔偵丄
        4 field 抶墑偲偟偰偄傞丅乮偙偺忬懺偱偼丄偢偭偲丅乯
        偙偺偨傔丄Bus Toggle Off 偱 DmeWipe 偵 PinP 偺條側僷僞乕儞傪
        慖戰偡傞偲丄僼僃乕僟乕偺怳傝愗傝帪偵丄僔儑僢僋乮堦弖丄Bkgd 偺媡夋乯
        偑弌傞偙偲偑偁傞丅


3. Additional PP

    丒4.5ME 峔惉偵偼側傜側偄丅
    丒OUT17-22 偼屌掕傾僒僀儞偲側傞丅

       ----------------------------------
         OUT  |  Assign  (when DSK Mode)
       ----------------------------------
        OUT17 | PP PGM   (PP PGM1)
        OUT18 | PP PGM   (PP PGM2)
        OUT19 | PP PVW   (PP KPVW1)
        OUT20 | PP CLEAN (PP KPVW2)
        OUT21 | PP KPVW  (PP CLEAN1)
        OUT22 | PRESET   (PP CLEAN2)
       ----------------------------------

    丒Add-PP 慜偺愝掕偱忋婰傾僒僀儞傪慖戰偟偰偄偨懠偺 OUT 偼 No Assign 偵側傞丅
    丒PP 偺儕僄儞僩儕偼 OUT23,24 偵傾僒僀儞偟偨弌椡偱偟偐慖戰弌棃側偄丅
      Edit PVW 摍丄PP 偺儕僄儞僩儕偑昁梫側弌椡偼 OUT23,24 偵傾僒僀儞偡傞偙偲丅


4. CCR

    丒DVS-9000/SF 偱儔僀僙儞僗傪僀儞僗僩乕儖偟偰偄側偄応崌偺弌椡偼曐徹奜丅
      (堦尒丄慺捠傝偟偨夋憸偑弌傞応崌偑偁傞偑丄埵憡偼曐徹偱偒側偄丅)

    丒CCR 1/2 偱偼 Input Phase Adjust 偼柍岠偲側傞丅


5. Output Setup

    丒EngSetup Output V Blank Mask 偺抣偼丄User Define 偝傟偨 Setup
      偱婲摦偟偨応崌丄價僨僆僼僅乕儅僢僩偵娭學側偔 User Define 抣偲側傞丅
      乮巇條乯
      價僨僆僼僅乕儅僢僩偺曄峏屻偵偼拲堄偑昁梫丅


6. DME 4ch Proc.K       仮c1 捛壛       2004.9.27

   丒愱梡 I/F 愙懕偺 DME 傪 2戜巊梡偡傞応崌丄
     曅曽偺 DME 偱 Proc.K 傪 4ch 僐儞僶僀儞偱巊梡偡傞偲丄
     巆傝偺 DME 偱偼丄2ch 僐儞僶僀儞偑嵟戝偱丄3ch,4ch 僐儞僶僀儞偼偱偒側偄丅
     Switcher 撪晹偺僶僗(DmeUtil)傪巊偄愗偭偰偟傑偆偨傔丅


7. Frame Memory Animation       仮c2 捛壛       2004.10.14

     丒FM Animation 偺 Create Keyframe 偍傛傃 Append Keyframe
       婡擻傪幚峴偡傞偲偒偼丄Panel 柺偺 EFF 儕乕僕儑儞慖戰儃僞儞
       偺偆偪奩摉偡傞 User 儕乕僕儑儞偺傒傪 ON 偵偟丄娭學偺
       柍偄儕乕僕儑儞偼 OFF 偵偡傞偙偲丅
       偙傟傪峴傢側偄偲丄Animation 僼傽僀儖偑惓偟偔惗惉偝傟側偄丅

     丒Create KF 偺枃悢(Duration)偼丄99 偑嵟戝抣丅偦傟埲忋傪巜掕偟偰傕丄
       99 枃偲偟偰摦嶌偡傞丅


8. Transition   仮c5 偱捛壛

  (1) One Time Pst Color Mix 捈慜偺 Pattern Limit 偼丄奐巒捈慜偺忬懺偑 On
      傑偨偼 Green 偱偁偭偰傕丄捈屻偼 Off 偲側傞丅


9. Wipe         仮c5 偱捛壛

  (1) 720P/59.94 偱偼丄儌僨傿僼傽僀帪偺摦嶌 (娷丄庢傝愗傝) 偼曐徹偟側偄丅
  (2) Rotary Wipe 慖戰帪丄Key Type 傪 Wipe Pattern 偵偡傞偲岆摦嶌偡傞丅
  (3) Resume 摍偺婲摦偱 Wipe 偺 Transition 搑拞偲側傞応崌丄
      Transition 偼惓偟偔摦嶌偟側偄丅
      悢夞僼僃乕僟乕傪怳傝偒傞偲丄惓忢摦嶌偵側傞丅  仮c13 捛壛


10. DME Link (Proc Key / DME Wipe)         仮c5 偱捛壛

  (1) Common Local Trans 偺偄偢傟偑偑 DME Wipe 偺帪丄Auto Trans 傪
      摨帪墴偟 (Trans Rate 偼摨偠) 偡傞偲丄Trans 廔椆帪偵丄夋偵僔儑僢僋偑
      敪惗偡傞丅
  (2) 僼僃乕僟乕傪搑拞偺忬懺偱 DME Wipe 傪 Resume 摍偱婲摦偟偨捈屻偺摦嶌偼
      曐徹偟側偄丅
      Auto Trans Start 傪偡傞偐丄僼僃乕僟乕儗僶乕傪壗搙偐怳偭偰偐傜巊梡偡傞
      偙偲丅
  (3) DME Wipe 偺忬懺偺傑傑 Resume 偟偨捈屻偺摦嶌偼曐徹偟側偄丅
      暅婣偵偼椺偊偽丄堦扷丄Trans Type 傪 DME Wipe 偵偟偰丄 Wipe 偵偡傞丅
  (4) MVE 偺 Fore/Back 傪暿慺嵽偵偡傞偲丄夞揮帪 Key Source 偑 Split 偵側傞丅
  (5) DME Wipe 偺 LPVW 側偳僾儗價儏乕夋偼惓偟偄夋偵側傜側偄丅
      DME Wipe Frame In/Out 傪幚峴拞偺 LPVW 偺夋偼丄DME 栠傝夋偑巊傢傟傞応崌
      偲丄DME 旕宱桼偺夋偑巊傢傟傞応崌偑偁傞丅(Transition 姰椆帪偵 PinP 忬懺
      偲側傞応崌偱傕丄LPVW 偼 PinP 偵側傞偲偼尷傜側偄丅)
  (6) Common / Local Trans 偺 Key 偱 DME Wipe Frame In/Out 傪巜掕偟偰丄
      Preview 偱 DME V 傪慖戰偡傞側偳偵傛傝 DME 栠傝夋傪尒傞応崌丄
      僉乕僆僼忬懺偱偁偭偰傕丄DME 栠傝夋偼僉乕僆儞忬懺偺夋偲側傞応崌偑偁傞丅
  (7) Common / Local Trans 偺偄偢傟偐偑 DME Wipe 偺応崌丄Common 偍傛傃 Local
      偺 Trans 奐巒傑偨偼廔椆偑 4僼傿乕儖僪撪偵廳側偭偨応崌丄夋偵僔儑僢僋偑
      敪惗偡傞応崌偑偁傞丅
  (8) DME Wipe 拞偵 Bus Toggle On/Off 傪愗傝姺偊傞偲丄岆摦嶌偡傞丅
      偙偺応崌丄堦搙懠偺 Trans Type (椺 Mix) 傪慖戰偟偰偐傜丄DME Wipe 傪慖戰
      偡傞偙偲丅
  (9) 儅僋儘摍偱 DME Wipe丄Proc.K 偑娭學偡傞憖嶌偼丄椬愙偡傞憖嶌偲偺娫偵 2僼
      儗乕儉埲忋偺娫妘偑昁梫丅(娫妘偑柍偔偰傕摦偔応崌傕偁傞偑丄僔儑僢僋偑弌
      傞偙偲偑偁傞丅)
  (10) (Kf 側偳偱) Trans 偺搑拞偐傜摦偐偟巒傔傞偲丄Flip 偺夋偺愗傝懼傢傝偑偢
       傟傞偙偲偑偁傞丅
       User Program 偱 Flip Pattern 傪嶌傞応崌偼丄Flip 揰偑 KF 偺拞墰偵棃傞
       偙偲偑朷傑偟偄丅惓妋偵拞墰偱側偔偲傕丄椉抂偺 10% 埲奜偺埵抲側傜偽丄
       捠忢偺摦嶌 (Trans 偵拞抐側偟偺応崌) 偵偼丄傎偲傫偳栤戣偼側偄丅
       偟偐偟丄僼僃乕僟丒儗僶乕偵傛傞憖嶌側偳偱丄婓偵栤戣偑弌傞偙偲偑偁傞丅
  (11) User Program 僷僞乕儞偺 Trans Mode 傪儊僯儏乕偐傜曄峏偡傞応崌丄
       DME Wipe 幚峴拞偵偼斀塮偝傟側偄丅堦搙 Trans Type 傪 DME Wipe 埲奜偵
       曄偊偰丄DME Wipe 傪慖戰偟側偍偡偙偲丅

  (12) Xpt Hold 偵娭偡傞惂尷帠崁 [mvs-soft:42213]    仮c6 偱捛壛

    丒DME1V,DME1K 摍偺壖憐僶僗偺 Xpt Hold
      憖嶌偟偰傕柍岠丅
      墴壓偡傞偲揰摂偡傞応崌偑偁傞偑丄岠壥偼丄側偄丅

    丒SDI I/F 偱偺 Aux Bus 偺 Xpt Hold
      3rd/4th ch 偲偟偰巊傢傟傞応崌偼桳岠丅

      1st/2nd ch 偺僶僗偵巊傢傟傞応崌偼丄
      ME 偺僶僗偵儕儞僋偡傞偨傔丄Xpt Hold 偟偰傕岠偐側偄丅
      ME 偺僶僗偱 Xpt Hold 墴壓偡傟偽丄Hold 偝傟傞丅

    丒Snapshot Attribute Xpt Hold
      DME 3rd ch 偺僜乕僗僶僗偑丄側偄丅乮慖戰丒愝掕偱偒側偄丅乯

    丒KF Path Xpt Hold
      DME 3rd ch 偺僜乕僗僶僗偑丄側偄丅乮慖戰丒愝掕偱偒側偄丅乯

  (13) SDI I/F DME 偺惂尷               仮c16 偱捛壛
    丒SDI I/F 偱偼丄栠傝宯摑偑 1宯摑偟偐柍偄偺偱丄
      DME Wipe 偲 Proc.K 側偳丄2婡擻傪摨帪偵偼巊偊側偄丅
    丒摨堦 ME 撪偱 SDI I/F DME 偲愱梡 I/F DME 傪摨帪偵巊偆偙偲偼弌棃側偄丅
        偨偩偟丄 V7.20 埲崀偼 Setup 偵捛壛偟偨 <KeyDmeIfSimul> 偵傛傝丄
        愱梡 I/F 偺 Proc.K DME 偲 SDI I/F 偺 Proc.K DME 偲傪丄摨堦 ME 撪偱
        摨帪偵壜擻偲丄偡傞偙偲偑偱偒傞丅


11. Copy / Swap         仮c5 偱捛壛

  (1) Keyer Copy 傪偡傞偲丄偦偺 Local Wipe 傕僐僺乕偝傟偰偟傑偆丅
  (2) Keyer Copy 偱丄Proc Key 偼僐僺乕偝傟側偄丅


12. Keyframe            仮c5 偱捛壛

  (1) Kf 悢偼巇條偺 1000 Keyframe 偐傜丄500 Keyframe 偵曄峏丅(V1.10偺傑傑)
  (2) Register Delete Undo 偼枹僒億乕僩丅
  (3) Wipe 偲 Trans 偺 Kf Path 傪堎側傞傕偺偵偟偨応崌丄Wipe 偺僒僀僘偼
      Trans (Fader) 偱偼側偔丄Wipe 偺愝掕偵偟偨偑偭偰摦嶌偡傞丅
  (4) DME 傪巊偭偨 KF 揰偼丄慜屻偺 KF 揰偲偺娫妘偑 3僼儗乕儉埲忋昁梫丅
  (5) Load 偟傛偆偲偡傞 Keyframe 僼傽僀儖偵傛偭偰丄Kf 悢偺惂尷抣 (500) 偑
      挻偊傞応崌丄僄儔乕偵側傞丅偙偺応崌丄僄儔乕偵側偭偨儗僕僗僞傪 Effect
      儊僯儏乕偱 Delete 偡傞偙偲丅偟側偄応崌丄晄嬶崌傪惗偠傞壜擻惈偑偁傞丅
  (6) Xpt Hold 傪 Key Disable 偵愝掕偟偰 Keyframe 傪幚峴偡傞偲丄
      僗僀僢僠忣曬偼曄壔偟側偄偑丄傾僫儘僌忣曬偼曄壔偟偰偟傑偆丅

  (7) Shotbox丄Flexi Pad 偵娭偡傞惂尷    仮c6 偱捛壛

      Recall & Run 傪桳岠偵偟偨忬懺偱 6 夞埲忋楢懕偟偰 Shotbox 儃僞儞傪
      墴偡偲丄Run 偼峴偄傑偡偑 Recall 偼峴傢側偄応崌偑偁傝傑偡丅
      偙傟偼 Recall 僐儅儞僪傪僶僢僼傽儕儞僌偡傞儊儌儕検偵傛傞惂尷偱偡丅(V5.11)


13. Frame Memory        仮c5 偱捛壛

  (1) Ss Recall 偡傞応崌丄Bkgd 傪 Field Freeze 偟偰夋憸壛岺拞偺忬懺傪屇傃
      弌偡偵偼 5僼儗乕儉丄偦偺懠偺応崌偼 2僼儗乕儉埲忋娫妘傪娫妘傪奐偗側偄偲丄
      摦嶌曐徹偝傟側偄丅<巇條>
  (2) 僗儖乕夋傪 Reposition 拞偵 Field Freeze 偡傞偲丄堦弖 Reposition 偑夝彍
      偝傟傞丅
  (3) Frame Memory 偼丄儕僄儞僩儕慖戰偱儖乕僾偱偒偰偟傑偆丅<巇條>

  (4) FM HDD    仮c6 偱捛壛

    丒懳墳 HDD 偼 Maxtor OneTouch III, Lacie d2 Quadra 偺傒丅
    丒2戜偺 HDD 傪岎屳偵愙懕偡傞偲丄婬偵 MY 偑僴儞僌傾僢僾偡傞丅
      Lacie d2 Quadra 偲 OneTouch II 偺慻崌偣偱尰徾傪妋擣丅

  (5) FM Ancillary    仮c11 偱捛壛, 仮c14 偱曄峏

    丒Unit Config 偑 FM Data = Reverse 偲 FM Ancillary = On 偺椉棫偼晄壜丅
      摨帪偵愝掕偝傟偨応崌丄FM Data 偑 Normal 偲側傞丅
    丒埲壓偺憖嶌傪偟偰偄傞娫偼丄僲僀僘偑婰榐/嵞惗偝傟傞応崌偑偁傞丅
      - Menu 偵僾儘僌儗僗僶乕偑弌傞張棟傪幚峴偟偨帪
      - Keyframe 偺曇廤拞
      - Keyframe 偺 Run 拞
      - FM > Still > Create Keyframe 儊僯儏乕 (Menu 2515) 憖嶌拞
      - FM > File 儊僯儏乕 (Menu 254x) 憖嶌拞
      - FM > Folder 儊僯儏乕 (Menu 255x) 憖嶌拞
      - FM > External HDD 儊僯儏乕 (Menu 256x) 憖嶌拞
      - Register 儊僯儏乕 (Menu 6xxx) 憖嶌拞
      - File 儊僯儏乕 (Menu 71xx) 憖嶌拞
      - Eng Setup > System 儊僯儏乕 (Menu 731x) 憖嶌拞
      - Eng Setup > Switcher 儊僯儏乕 (Menu 733x) 憖嶌拞
    丒埲壓偺憖嶌偱偼僲僀僘偑敪惗偡傞偙偲偑偁傞丅
      - Freeze (Record) Enable 偺 On/Off 愗懼
      - Freeze (Record) Enable On 拞 (傑偨偼 Record 拞) 偺 FM Src XPT 愗懼
      - AUX 偺 XPT 愗懼
      - Black 佁 Still, Black 佁 Clip, Still 佁 Clip 偺愗懼
      - Clip 佁 Clip 愗懼 (Embedded Audio 偺巊梡 ch 偑堎側傞 Clip 偺応崌偺傒)
      - Clip 偑5偺攞悢偱側偄僼儗乕儉悢偺帪偺 Loop Play (摿掕僼僅乕儅僢僩偺傒)
          奩摉僼僅乕儅僢僩 :  480i/59.94, 720P/59.94, 1080i/59.94
                              1080PsF/23.975, 1080PsF/29.975
      - Record 偟偨 Clip 傪曇廤 (夋偺憓擖/嶍彍) 偟偨応崌偺 Clip Play
        (嶍彍偼丄拞娫偺嶍彍偺傒奩摉丅愭摢傗枛旜偺嶍彍偩偗側傜丄敪惗偟側偄)
    丒MVS-8000A/ASF 偱偼丄FM Ancillary 傪巊梡偱偒傞偺偼 FM1/FM3/FM5/FM7
      偺傒偵惂尷偝傟傞丅
    丒僆乕僨傿僆僒儞僾儕儞僌廃攇悢偼價僨僆摨婜偺 48kHz 偺傒丄摦嶌曐徹偡傞丅
      僆乕僨傿僆僋儘僢僋埵憡僨乕僞偐傜僒儞僾儕儞僌僋儘僢僋傪拪弌偟偰偄傞
      婡婍偺摦嶌偼曐徹偟側偄丅

  (6) FM 2枃栚婎斅 (Ext Clip)  仮c11 偱捛壛

    丒揹尮搳擖帪丄儊僯儏乕偐傜偺儕僙僢僩帪丄2枃栚婎斅傪擣幆偟側偄傛偆側忬懺
      偲側傞応崌偑偁傞丅
        - FM 儊僯儏乕偱丄Ext 懁偺巆傝枃悢偑昞帵偝傟側偄
        - Menu 7316.1 偺 Detail Information 偱 FM 婎斅偑昞帵偝傟側偄
      偙偺応崌偼丄僗僀僢僠儍乕傪嵞婲摦偡傞昁梫偑偁傞丅

  (7) 720P/59.94, 720P/50 僼僅乕儅僢僩帪偺 Clip 摦嶌  仮c14 偱捛壛

    丒婏悢枃偺 Still 偱峔惉偝傟偨 Clip 偺摦嶌偼曐徹偟側偄丅
      昁偢嬼悢枃偺 Still 偱峔惉偝傟偨 Clip 傪巊梡偡傞偙偲丅傑偨丄
      Clip 傪峔惉偡傞 Still 傪嶍彍偡傞応崌丄昁偢2枃偢偮嶍彍偡傞偙偲丅
    丒Create Key Frame 偱嶌惉偟偨 Animation 偼 Progressive 摦嶌偟側偄丅
    丒婏悢僼儗乕儉傊偺堏摦偼偱偒側偄丅(Timecode 巜掕堏摦丄Cueup)
    丒婏悢僼儗乕儉偱 Stop 偟偨応崌丄僒儉僱僀儖偲幚夋憸偑僘儗傞偙偲偑偁傞丅
    丒V7.20 傛傝傕慜偺僶乕僕儑儞偱曐懚偝傟偨 Clip 傪 V7.20 埲忋偱嵞惗偡傞
      偲丄2攞懍偱嵞惗偝傟傞丅
    丒Clip Auto Play 懏惈偺偮偄偨 Snapshot 傪 Recall 偟偨応崌丄Clip 偺
      愭摢僼儗乕儉偼 Recall 偝傟偢丄2僼儗乕儉栚偐傜 Play 偑奐巒偝傟傞丅

  (8) FM Data Port  仮c14 偱捛壛

    丒FM Data Port 偵摨帪偵愙懕偱偒傞僋儔僀傾儞僩 (Menu, System Manager) 偼
      SWR 1戜偵偮偒1偮偲偡傞丅


14. Switch Timing       仮c5 偱捛壛

  (1) Legacy I/F 偵偍偗傞 Switch Timing 偼丄慡僐儅儞僪偵揔梡偝傟傞丅<巇條>
      (儃儕儏乕儉宯偺僐儅儞僪偵傕揔梡偝傟傞丅)
  (2) Auto Trans 偼奐巒僞僀儈儞僌傪崌傢偣傞丅<巇條>
     偙傟偵傛傝丄Trans 姰椆帪偺 Xpt 愗懼偊偼巜掕偺僼儗乕儉悢偺 1僼傿乕儖僪
     庤慜偱峴傢傟傞偙偲偵側傝丄Bus Link 摍偺捛壛幚峴偼丄Switch Timing 偲
     崌傢側偔側傞丅
  (3) Trans Type == Cut 帪偺 Fader Lever 偵傛傞僞僀儈儞僌偼曐徹偟側偄丅<巇條>
  (4) Fader Lever 偵傛傞 Trans 姰椆偺僞僀儈儞僌偼曐徹偟側偄丅<巇條>
  (6) DME Link 偱惗偠傞愗懼偊僞僀儈儞僌偼丄DME 懁偺惂屼偵埶懚偡傞丅<巇條>
      (MVS 懁偱偼壗傕惂屼偟側偄丅)


15. GPI Output (GPI Link)       仮c5 偱捛壛

  (1) 巜掕偟偨 Action 偑惂栺帠崁摍偱丄幚峴偝傟側偔偰傕 GPI Output 偼摦嶌偡傞
      応崌偑偁傞 丅<巇條>


16. Keyframe : Transition 傪 Modify 偟偨応崌偺曐徹奜偺寢壥偵偮偄偰
        仮c5 偱捛壛

  (1) 幚嵺偺摦嶌偼丄椺偊偽 KF 娫偱 Key 偑 On 偺曽岦偵 Transition 偑恑傫偱傕丄
      KF 揰偵摓払帪偵丄晄楢懕側摦嶌 (KEY Off 偵側偭偨傝偡傞傛偆側摦嶌) 傪偡傞丅

  (2) Fader 傪堦扷庢傝愗偭偰丄偝傜偵搑拞偵偟偨応崌偺摦嶌丅

  (3) KF 偺奐巒廔椆揰偱 Fader 偑晜偄偰偄傞帪偵丄Fader 傪庢傝愗傞摦嶌偱 KF 偺
      拞娫揰傪 Modify 偡傞応崌丅

  (4) Transition 傪孞傝曉偟偰偄傞 Effect 偺丄嵟弶偺 KF 揰偺 Fader 傪庢傝愗偭偰
      (偦偺 KF 傪傂偲偮偩偗) Modify 偟偨応崌偺丄埲崀偺 KF 偱偺 Trans 偺摦嶌丅
      (寢壥偑斀揮偡傞傛偆側 DVS 偺條側摦嶌偼峴傢側偄丅)

  (5) Trans Type = Wipe 偐偮 PTN Limit = On 偺 KF 傪丄Type = Mix 偵偡傞丅
      (偁傞偄偼 Trans Type = Wipe 偺帪偵 PTN Limit 傪 On 偵偡傞丅)

  (6) 暋悢 KF 偺 Modify 偵娭偟偰 Wipe 偺 Modifyer 傪曄峏偟偰憡懳抣 Modify 傪
      峴側偭偨帪偵丄Modify 懳徾偺 KF 揰偵 Wipe Transition 傪姰椆偡傞暔偑偁傞
      偲丄Transition 偺姰椆偑憗偐偭偨傝抶偐偭偨傝偡傞丅(椺丗Border, Positioner)
      偦偺応崌丄Wipe Transition 偑姰椆偡傞 KF 揰偵 GO TO KF 傪峴偄丄
      (扨堦) KF Modify 傪峴偆帠偱惓偟偔嵞尰偱偒傞傛偆偵側傞丅


17. Side Flags    仮c6 偱捛壛

  (1) DME-Wipe 偺僩儔儞僕僔儑儞偱偼丄Side Flags 偺棤懁偱偼側偔丄
      庤慜懁傪 DME 偺栠傝夋偑捠夁偡傞丅偙傟傪巇條偲偡傞丅(V5.0)
      (AutoCrop 偟偨 墶曽岦 DmeWipe 側偳偑暘偐傝傗偡偄丅)

  (2) DME EXT V Bus 偺 SideFlags On/Off 傪庤摦憖嶌偡傞庤抜偑側偄丅
      Auto SideFlags 偱偺帺摦 On/Off 偺傒偑僒億乕僩偝傟偰偄傞丅

  仮c12 偱捛壛
  (3) Side Flags 偵偰丄DME Wipe 偺 4:3 Crop 帪偺暆偑嬐偐偵嫹偔丄
      Side Flags 偲偺娫偵寗娫偑弌棃傞丅
      see BRS-10389

  仮c12 偱捛壛
  (4) Side Flags 偺暆偑椉僒僀僪偱堎側傞丅
      see BRS-10371


18. Multi PGM Mode 2 偵娭偡傞惂尷    仮c6 偱捛壛

  丒Multi PGM Mode 偺惂尷偼 Multi PGM Mode 2 偵傕揔梡偝傟傞丅
    (乽2. Multi PGM Mode 偵娭偡傞惂尷乿傪嶲徠丅)
  丒棙梡偡傞偨傔偵偼 CA 婎斅偺 Main CPU 偑 DT 偱偁傞偙偲偑昁梫丅

18-1. BB-SRAM 偵娭偡傞惂尷

  BB-SRAM 偺婰壇懳徾偵 Sub ME x 4 偮暘偑憹壛偡傞偨傔丄V5.21 傑偱偺僨乕僞偲
  V5.30 埲崀偺僨乕僞偵偮偄偰 BB-SRAM 忋偱惍崌偑庢傟側偔側傞偨傔丄
  V5.21 埲慜偺僶乕僕儑儞偐傜丄V5.30 埲崀偺僜僼僩偵僶乕僕儑儞傾僢僾偟偰丄
  僔僗僥儉傪嵞婲摦偡傞偲 BB-SRAM 忋偺僨乕僞偑徚偊偰側偔側傞丅
  懳徾偼師偺捠傝丅

    - Snapshot
    - Keyframe
    - Key Snapshot
    - Wipe Snapshot
    - DME-Wipe Snapshot
    - Key Memory
    - Video Process Memory

  偙偺偨傔丄偙偺傛偆側僶乕僕儑儞傾僢僾傪峴偆応崌偵偼丄
  僶乕僕儑儞傾僢僾慜偵 HDD 側偳儊僨傿傾偵奩摉僼傽僀儖傪僙乕僽偡傞偙偲丅
  僔僗僥儉傪僶乕僕儑儞傾僢僾偟偨屻偵僙乕僽偟偨儊僨傿傾偐傜儘乕僪偡傟偽丄
  廬棃偺僨乕僞傕巊梡偡傞偙偲偑壜擻偲側傞丅

  CA 婎斅偺 Main CPU 偑 DR 偺応崌偼丄偙偺棟桼偵傛傝 BB-SRAM 偱偺僨乕僞偑
  夡傟傞偙偲偼側偄 (ME 偼 4 偮偺傑傑) 偑丄DR 偺応崌偱傕忋婰偺傛偆偵僨乕僞傪
  堦搙儊僨傿傾偵媧偄忋偘傞庤弴傪悇彠偡傞丅

18-2. Xpt

  (1) Xpt 偺儕僄儞僩儕偵娭偡傞惂尷 (SWR)

    摨堦 ME 偱偺 Main -> Sub 傕偟偔偼 Sub -> Main 傊偺儕僄儞僩儕偼弌棃側偄丅
    摨堦 ME 偱偺 Main -> Sub 傕偟偔偼 Sub -> Main 傊偺儕僄儞僩儕傪庢傞応崌偼
    働乕僽儖偱鉃懱偺奜傪夞偡昁梫偑偁傞丅

    仮c15 4峴捛壛
    V7.20 偐傜偼丄MP2 Reentry Enable 愝掕偲偡傞偙偲偱壜擻偩偑丄
    儕僄儞僩儕偟偨夋偼 1H 棊偪乮壓偑傞乯偲側傞丅
    MP2 Reentry Enable 愝掕偺応崌丄摨堦 ME 撪偺儕僄儞僩儕偼丄
    夋偑夡傟傞応崌偱傕嬛巭偝傟側偄偺偱丄憖嶌偱拲堄偡傞昁梫偑偁傞丅
    懠偺 ME 傪宱桼偡傞応崌傕摨條丅

18-3. Transition

  (1) Main/Sub 嫟桳 Keyer 偺 Common Trans 憖嶌偵娭偡傞惂尷 (SWR)

    椺偊偽埲壓偺傛偆偵 Main 偲 Sub 偺 Panel 偑偁傝丄
    Swer 偺 Main 偲 Sub 偱 Key2 傪嫟桳偟丄
    Main 偲 Sub 偺 NextTrans 偵 Key2 傪慖戰偟偰偄偨偲偡傞丅
    偙偺偲偒 Main Panel 偺 CommonTrans 憖嶌偱 Key2 傪憖嶌拞偱偁偭偰傕丄
    Sub Panel 偺 CommonTrans 憖嶌偱 Key2 偺憖嶌偑弌棃偰偟傑偆丅
    偙偺偨傔 Key2 偑僕儍儞僾側偳偟偰偟傑偆丅

                劇劅劅劅劅劅劉
                劆Main Panel劌劅劉
                劋劅劅劅劅劅劊  劆     Main/Sub
                                劆  劇劅劅劅劅劅劉
                                劌劅劎Swer (Mix)劆
                                劆  劋劅劅劅劅劅劊
                劇劅劅劅劅劅劉  劆
                劆Sub Panel 劌劅劊
                劋劅劅劅劅劅劊

  (2) Local Trans 憖嶌偵娭偡傞惂尷 (PNL)

    Main/Sub 偺 Key Assign 偵娭學側偔丄Panel Delegation 偑
    Main/Sub/Main&Sub 偺儌乕僪偱偁偭偰傕丄忢偵 LocalTrans 憖嶌偑壜擻偲側傞丅
    Main/Sub 偺 Key Assign 偲 Panel Delegation 偑楢摦偟偰丄
    Key 憖嶌偵惂尷傪偐偗傞傛偆側偙偲偼偟偰偄側偄丅(尰忬偺巇條)

  (3) Tally 惗惉偵娭偡傞惂尷 (SWR)

    Main/Sub 扨埵偱僞儕乕忣曬傪惗惉偟側偄丅
    廬棃捠傝 ME 扨埵偱 僞儕乕忣曬傪惗惉偟丄捠抦偡傞丅
    Main/Sub 扨埵偱僞儕乕忣曬傪惗惉偟偨偄偲偒偼丄
    System Tally 傪梡偄傞丅

  (4) Panel Delegation 愗懼偵傛傞僼僃乕僟乕儗僶乕憖嶌偵娭偡傞惂尷 (PNL丄SWR)

    丒Main/Sub 摨帪憖嶌偼丄
      僗僀僢僠儍乕偺 Main 偲 Sub 偺 Setup 偑堎側傞応崌丄
      傑偨丄僗僀僢僠儍乕偺 Main 偲 Sub 偺 Setup 偑摨偠偱偁偭偰傕丄
      2 僗僩儘乕僋偺僩儔儞僕僔儑儞 (Pst Color Mix丄Pattern Limit) 偺応崌偼
      摦嶌傪曐忈偟側偄丅Snapshot丄Keyframe 傪娷傓丅
      (尰忬偺 ME 儕儞僋婡擻偲摨摍偺惂尷偑偁傞丅)

    丒Panel Delegation 愗懼偼丄
      2 僗僩儘乕僋偺僩儔儞僕僔儑儞搑拞偱偼曐徹偟側偄丅

    丒僼僃乕僟乕儗僶乕偑搑拞偵偁傞忬懺偱 Panel Delegation 傪愗傝懼偊偨応崌丄
     夋偺楢懕偼曐徹偟側偄丅

    仸 Panel 偺 Delegation 愗懼 偼僩儔儞僕僔儑儞偑姰椆偟偰偄傞忬懺偱
       峴偆偙偲傪悇彠偡傞丅

18-4. Wipe

  (1) Sub ME Wipe 偵娭偡傞惂尷 (SWR)

    Sub ME Wipe 偵偮偄偰偼丄Add-PP (0.5ME) 傗 MFS PP 偺 Wipe 偺傛偆偵
    惂尷偑偁傞丅(摨條偺夞楬傪棳梡偟偰偄傞偨傔丅)
    椺偊偽丄

      丒Wipe Position 傪堏摦偡傞偲 Wipe 僒僀僘偑曄傢傞丅
      丒Wipe Border 偺暆偑 P/P 楍偲 M/E 楍偱堎側傞丅

    側偳偱偁傞丅

18-5. Snapshot

  (1) Panel 偺摦嶌儌乕僪偑 Main&Sub 偺応崌偺 Common Fader Lever 偵娭偡傞惂尷

    Main ME 偲 Sub ME 偱 Setup 偑堎側傞偲偒丄Snapshot Recall 捈屻偺
    Common Fader Lever 偺摦嶌偼曐徹偟側偄丅
    傑偨 Setup 偑摨偠偱偁偭偰傕 Recall 偟偨捈屻偵 2 僗僩儘乕僋僩儔儞僕僔儑儞傪
    慖戰偟偨忬懺偲側偭偨応崌偵偼丄Common Fader Lever 偺摦嶌傪曐徹偱偒側偄応崌偑
    偁傞丅

  (2) Sub Common DME-Wipe (Sub ME Common 偺 DME-Wipe) 偵娭偡傞惂尷

    Sub Common DME-Wipe 偼 Snapshot 偺懳徾奜偱偁傞丅
    Store 傕 Recall 傕偝傟側偄丅

  (3) DME EXT V Bus 偵娭偡傞惂尷

    DME EXT V Bus 偼 Main ME 偲 Sub ME 偺嫟桳儕僜乕僗偱偁傞偨傔丄
    Main 懁 偱 DME EXT V Bus 傪巊偆傛偆側 DME-Wipe 僷僞乕儞傪慖戰偟偰偄傞偲偒偵
    Sub 懁偱 Ss Recall 側偳傪峴偆偲 DME EXT V Bus 傕堦弿偵愗傝懼偊偰偟傑偆偨傔丄
    Main 懁偺夋偵塭嬁偑弌偰偟傑偆丅

  (4) Sub Region 巜掕偺 Store/Recall 偵娭偡傞惂尷    仮c10 偱捛壛

    仦 Recall ME Config 偑 Enable 偺帪
       ME Config 偑 MP2 mode 偱側偄帪偺 Sub Region 巜掕偱偺 Recall 摦嶌偼
       曐徹偱偒側偄丅
       ME Config 偑 MP2 mode 偱側偄 Snapshot 僨乕僞傪 Sub Region 傊 Copy 偟丄
       Recall 偟偨応崌傕摨條丅
       嫟捠儕僜乕僗晹暘乮Bus, Key乯偟偐 Recall 偝傟側偄丅
       see [mvs-soft:55895]

    仦 Recall ME Config 偑 Disable 偺帪
       堎側傞摦嶌儌乕僪偱嶌惉偟偨 Snapshot 僨乕僞偺 Recall 摦嶌偼曐徹偱偒側偄丅

18-6. Keyframe

  婎杮揑偵 18-5. Snapshot 偲摨條偱偁傞丅

18-7. Master Ss丄Shotbox Ss

  Main/Sub 偺摨帪 Snapshot Recall 偵偮偄偰偼丄
  Main 偲 Sub 偺儗僕僗僞斣崋偑堦抳偡傞応崌偺傒摦嶌傪曐徹偡傞丅

仮c7
18-8. DME-Wipe 

  (1) DME-Wipe 偺 Main/Sub 摨帪巊梡 (BRS-14761丄[mvs-soft:47194])

    椺偊偽丄

      ME Main                             ME Sub
      BKGD丗DME(FlipTumble 埲奜) + KEY    BKGD丗DME(FlipTumble)

    偲偟偨偲偒丄ME Main 偺僩儔儞僕僔儑儞偱 BKGD 偲 KEY 偑偢傟傑偡丅
    FlipTumble 宯埲奜偺 DME-Wipe 僷僞乕儞偱偼抶墑惂屼傪峴偄傑偡偑丄
    FlipTumble 宯偺僷僞乕儞偱偼抶墑惂屼傪峴偄傑偣傫丅
    忋偺応崌丄

      Main Bkgd -> 抶墑惂屼
      Sub  Bkgd -> 旕抶墑惂屼

    偲側傝丄ME 慡懱抶墑偼峴偊偢丄Key 傕旕抶墑惂屼懳徾偲側傝丄
    Main Bkgd 偲 Key 偺夋偑偢傟傑偡丅

仮c7
19. Legacy I/F

19-1. Keyframe

  Legacy I/F 宱桼偱 Keyframe 憖嶌傪峴偆応崌丄Panel 偺 ID 偼昁偢 1 偲偡傞偙偲丅
  Legacy KF 僐儅儞僪 -> MVS KF 僐儅儞僪偺曄姺偱偼丄TableID 傪僛儘屌掕偲偟偰偄傞偨傔丅
  [mvs-soft:47293]丄BRS-14725


20. Clip Transition   仮c14 捛壛

  (1) Snapshot, Keyframe,

    丒Snapshot 偵偼僼僃乕僟乕抣偼婰壇偟側偄丅忢偵怳傝愗偭偨忬懺偲側傞丅
      僩儔儞僕僔儑儞搑拞偺忬懺傪婰壇偟偨 Snapshot 偺摦嶌偼曐徹偟側偄丅
    丒Keyframe 偵偼抣偼婰壇偝傟側偄丅忢偵 Clip Transition Off 偲側傞丅

  (2) Setup Load, 婲摦儌乕僪, Default Recall

    丒Setup Load 傗 Init Status Load 偱傕丄抣偼婰壇偝傟側偄丅
    丒婲摦儌乕僪偑 Resume 傗 User 偱傕丄抣偼婰壇偝傟側偄丅
      抣偼 Default Recall 偱傕婰壇偝傟側偄丅

  (3) 攔懠張棟

    丒Clip Transition 偱慖戰偟偰偄傞 FM Out 傪 FM 儊僯儏乕摍偐傜憖嶌偟偨
      応崌丄憖嶌偱偒偰偟傑偆丅(攔懠張棟偼偍偙側傢側偄)
    丒暋悢偺 M/E 偱丄摨偠 FM Out 傪懳徾偲偟偨 Clip Transition 傪慖戰偟偨
      応崌丄慖戰偱偒偰偟傑偆丅(攔懠張棟偼偍偙側傢側偄) 傑偨丄幚峴偟偨応崌
      偺摦嶌偼曐徹偟側偄丅

  (4) 僩儔儞僕僔儑儞摦嶌

    丒BKGD, Clip 偺 Start/Stop 偺愝掕偵傛傝丄晄姶懷偑弌棃傞偙偲偑偁傞丅
    丒BKGD Start/Stop 偺愝掕偵娭傢傜偢丄僩儔儞僕僔儑儞奐巒捈屻偐傜丄A/B
      Bus 嫟偵僴僀僞儕乕偲側傞丅(BKGD Transition Type 偑 User DME Wipe
      偺応崌傪彍偔)
    丒Clip Transition 偱曄峏偟偨 BKGD Transition 偺抣偼丄Clip Transition
      傪夝彍偟偰傕丄偦偺抣傪堷偒宲偖丅
    丒Clip Transition 慖戰拞偼丄Transition Rate 偼庤摦偱偼曄峏晄壜丅
    丒僼僃乕僟乕儗僶乕偑搑拞偵偁傞忬懺偱 Auto Transition 傪幚峴偟偨応崌
      偺摦嶌偼曐徹偟側偄丅

  (5) Clip 摦嶌

    丒Clip 偺壜曄懍嵞惗偼晄壜丅忢偵1攞懍偺 Normal/Reverse 嵞惗偲側傞丅
    丒FM 儊僯儏乕偺 Start/Stop TC 偼丄Clip Transition 偱偼柍岠偲側傞丅
    丒Ancillary Enable 偺 Clip 偼丄Clip Direction 偑 Normal 偺応崌偵偼
      壒偑嵞惗偝傟傞偑丄Reverse 偺応崌偵偼壒偼嵞惗偝傟側偄丅
    丒僀儞僞儗乕僗曽幃偺僼僅乕儅僢僩偺応崌丄Clip Direction 偑 Reverse
      偺応崌偵偼丄Clip Record 偟偨夋偼惓偟偔 Reverse 偟側偄偨傔丄CG 傪
      Import 偟偨夋傪巊梡偡傞昁梫偑偁傞丅
    丒Transition Rate 偺嵟戝抣 (999 Frame) 傪挻偊傞 Clip 偺摦嶌偼曐徹
      偟側偄丅傑偨丄Clip Start 傪曄峏偟偰丄Clip End 偑 Transition Rate
      偺嵟戝抣傪挻偊傞応崌偺摦嶌傕曐徹偟側偄丅

  (6) 枹僒億乕僩婡擻

    丒埲壓偺婡擻偲偺暪梡偼丄As is 摦嶌偲側傞丅
      - Split Fader
      - Pattern Limit
      - BKGD Transition 偺 2 Stroke 摦嶌
      - Advanced Tally Mode
    丒埲壓偺婡擻偼僒億乕僩偟側偄丅
      - M/E Link
      - Transition Preview

21. License 彂偒崬傒偲帺屓恌抐   仮c17 捛壛

  (1) License 彂偒崬傒偺幐攕

    V7.20 埲崀偱偼丄掕婜揑偵帺屓恌抐婡擻偵傛傞 EEPROM 彂偒崬傒傪峴偆偑丄
    偙傟偲摨偠僞僀儈儞僌偱 Licence 偺彂偒崬傒傪幚峴偡傞偲丄
    EEPROM 傊偺彂偒崬傒偵幐攕偡傞壜擻惈偑偁傞丅
    嵞婲摦屻丄儔僀僙儞僗夋柺偱峏怴偝傟偰偄側偄偺傪尒傞偙偲偱丄敾柧偡傞丅
    偦偺応崌丄傕偆堦搙彂偒崬傒憖嶌傪峴偭偰偄偨偩偔丅
    乮偦偟偰傕偆堦搙嵞婲摦偡傞丅乯


Appendix-1. CA-44 忋偺 DIP SW (S101) 偵傛偭偰摦嶌偡傞婡擻偵偮偄偰

  CA-44 忋偺 DIP SW (S101) 偵傛傞愝掕偼埲壓偺偲偍傝丅

  (1) 擖椡偺 TBC Window 偺暆傪崱傑偱捠傝偵僉乕僾偡傞婡擻

         SW1 | Keep Window
        -----|--------------------------------------------
         Off | Multi Format Option 偺桳柍偵傛偭偰曄壔偡傞
         On  | 廬棃偺 Window 暆偵屌掕偝傟傞

      On 偵偟偨応崌丄儕僄儞僩儕傪 4抜偵偡傞偲夋偑棎傟傞丅
      嬛巭張棟偼峴偭偰偄側偄偺偱丄塣梡偱偼拲堄偡傞昁梫偑偁傞丅

  (2) Multi Format Option 偺桳柍傪愝掕偡傞婡擻  (媽 SW2)
      仺 V3.00R3 偐傜帺摦専弌

  (3) Auto Trans Start 僐儅儞僪偺 Rate 巜掕傪柍帇偡傞婡擻丅

         SW3 | Auto Trans Start
        -----|----------------------------------
         Off | 僐儅儞僪偱巜掕偝傟偨 Rate 傪巊梡
         On  | 撪晹偱愝掕偝傟偰偄傞 Rate 傪巊梡

      傑偨丄僐儅儞僪僐乕僪偱丄Rate 巜掕傪偟偰偄側偄傕偺 (ByteCount = 2) 傪
      庴怣偡傞偲丄MVS 偼丄撪晹偱愝掕偝傟偰偄傞 Rate 傪巊梡偟偰 Auto Trans 傪
      幚峴偡傞丅<巇條>

  (4) 僶僢僋傾僢僾僋儕傾婡擻

         SW4 | Backup Clear
        -----|---------------------------------------------
         Off | 壗傕偟側偄
         On  | 僶僢僋傾僢僾僨乕僞 (SRAM丄Flash) 傪徚嫀偡傞

      徚嫀屻丄僔僗僥儉偼掆巭偡傞丅SW4 傪尦偵栠偟偰嵞婲摦偡傞偙偲丅<巇條>
      庡偵丄僶乕僕儑儞僟僂儞偟偰婲摦偟側偄応崌偵巊偆婡擻丅

      徚嫀張棟傪奐巒偟偨傜丄偦偺忬嫷傪埲壓偺傛偆偵 7SEG 偵昞帵偡傞丅
        嵍偺寘偼丄懳徾偲側傞僨乕僞傪帵偡丅
        丒'E' 側傜埲壓偺僨乕僞傪徚嫀偡傞丅
        - Resume 梡僨乕僞
        - Keyframe / Snapshot / Sub Snapshot 僨乕僞
        - Key Memory / Video Process Memory 僨乕僞
        丒'F' 側傜埲壓偺僨乕僞傪徚嫀偡傞丅
        - Setup Define 僨乕僞
        - Init Status Define 僨乕僞
        丒'G' 側傜埲壓偺僨乕僞傪徚嫀偡傞丅
        - System (Nv-Setup) 僨乕僞
        塃偺寘偼丄徚嫀偺忬懺傪帵偡丅
        丒'9' 乣 '1' 偼奐巒慜偺僇僂儞僩僟僂儞 (1昩娫妘) 傪帵偡丅
        丒'0' 偼徚嫀拞偱偁傞偙偲傪帵偡丅
        丒'-' 偼廔椆偟偨偙偲傪帵偡丅
        慡徚嫀張棟傪廔椆偟偨応崌偼 '--' 偲昞帵偡傞丅

      2004.9.1 捛婰 仺 僋儕傾偟偨屻偼丄Setup 偲 InitStatus 偺椉曽傪
                       Define 偟偰婰壇偡傞偙偲丅

  (6) KOA2 儌乕僪傪愝掕偡傞婡擻 (SW6)
      (V3.20R1_10 怴婡擻)
        (乽MVS-8000, MVS-8000/SF 偱乿仺 V3.21_1 偱偙偺忦審偼嶍彍)
        CCR 婎斅偑憰拝偝傟偰偄側偄応崌丄
        師偺傛偆偵撪晹張棟懍搙偵嶌梡偡傞丅

         SW6 | KOA2 儌乕僪
        -----|----------------------------------
         Off | CCR 婎斅偑側偗傟偽丄弶戙 KOA 偵懳墳偟偨掅懍捠怣偱摦嶌偡傞
         On  | KOA2 偱巊偊傞崅懍捠怣偱摦嶌偡傞

        CA 忋偺 KOA 婎斅 (2 枃) 傪彍偔丄僙僢僩撪偺 KOA 婎斅偑慡偰 KOA2 偵
        側偭偰偄傞応崌偵尷傝丄On 偵偡傞偙偲丅
        CCR 婎斅偑憰拝偝傟偰偄傞応崌偼丄偙偺 SW6 偵娭學側偔丄
        崅懍捠怣偱摦嶌偡傞丅
        崅懍捠怣偵偡傞偙偲偱丄僼僃乕僟傪怳偭偨帪偵夋偺曄壔偑 偑偨偮偔乮挼傇乯
        偺傪杊巭偡傞偙偲偑偱偒傞丅

        仮c8
        MVS-8000G/GSF 偼帺摦偱 KOA2 儌乕僪偲側傝傑偡丅
        V7.0 埲崀偺 KOA2 儌乕僪偼丄1394 捠怣曽幃傪曄峏偡傞偙偲偵傛傝丄
        A/ASF/G/GSF 偱丄偝傜偵崅懍捠怣傪峴側偆傛偆夵椙偝傟偰偄傑偡丅

  (7) 婲摦帪偵 BB-SRAM 偺僠僃僢僋僒儉傪僠僃僢僋偡傞偐 (V3.20R1_3乣)


  (8) DR / DT 敾暿僀儞僗僩乕儖傪婡擻偝偣傞偐    仮c3 捛壛       2005.04.08

      DR -> DT 傑偨偼 DT -> DR 偺傛偆偵 CPU 傪嵹偣曄偊傞応崌偵
      巊梡偡傞丅

         SW8 | DR / DT 敾暿僀儞僗僩乕儖傪婡擻偝偣傞
        -----|---------------------------------------------
         Off | 婡擻偡傞丅
         On  | 婡擻偟側偄丅


Appendix-2. Key 慺嵽偺儕僄儞僩儕忦審偵偮偄偰 V3.00

  儕僄儞僩儕忦審偼

    丒Keep Window 偺愝掕
    丒憰拝偝傟偰偄傞 M/E 椶 偺悢乮Add-PP娷傓乯
    丒Multi Format Option 偺桳柍
    丒M/E 椶偺 Xpt 偱 CCR 弌椡偑庢傜傟偰偄傞偐
    丒System Format

  偵傛偭偰丄埲壓偺傛偆偵曄壔偡傞丅
  乮尰嵼偼 FLOAT=OFF 屌掕乯

    (1)TBC_Window_Keep=ON 偺偲偒
      劕劒劒劚劒劒劒劚劒劒劒劚劒劒劒劚劒劒劒劒劒劒劒劚劒劒劒劒劒劒劒劖
      劔 ME 劔FLOAT 劔 MULT 劔  CCR 劔 1080/576/480 劔    720宯     劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  4 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔   LTD_4thME  劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔   LTD_4thME  劔   LTD_ALL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_ALL    劔   LTD_ALL *1 劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  3 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_FLK    劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔   LTD_FLK    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  2 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔    NORMAL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔    NORMAL    劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔   LTD_FLK    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔   LTD_FLK    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔   LTD_ALL    劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  1 劔  --  劔  --  劔  --  劔    NORMAL    劔    NORMAL    劔
      劘劒劒劤劒劒劒劤劒劒劒劤劒劒劒劤劒劒劒劒劒劒劒劤劒劒劒劒劒劒劒劗
        *1丗幚嵺偵偼嬛巭

    (2)TBC_Window_Keep=OFF
      劕劒劒劚劒劒劒劚劒劒劒劚劒劒劒劚劒劒劒劒劒劒劒劚劒劒劒劒劒劒劒劖
      劔 ME 劔FLOAT 劔 MULT 劔  CCR 劔 1080/576/480 劔    720宯     劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  4 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME*2劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME*2劔   LTD_ALL    劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔   LTD_4thME  劔   LTD_ALL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔   LTD_4thME  劔   LTD_ALL  *1劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL  *1劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  3 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔   LTD_3rdME  劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔   LTD_3rdME  劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔   LTD_FLK    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔   LTD_FLK    劔   LTD_3rdME  劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_3rdME  劔   LTD_ALL    劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  2 劔 OFF  劔 NONE 劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔    NORMAL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔    NORMAL    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔    NORMAL    劔    NORMAL    劔
      劔    劙劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔    劔  ON  劔 NONE 劔 NONE 劔    NORMAL    劔   LTD_FLK    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_FLK    劔   LTD_ALL    劔
      劔    劔      劦劅劅劅劸劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔 EXIST劔 NONE 劔    NORMAL    劔   LTD_FLK    劔
      劔    劔      劔      劦劅劅劅劸劅劅劅劅劅劅劅劸劅劅劅劅劅劅劅劮
      劔    劔      劔      劔 EXIST劔   LTD_FLK    劔   LTD_ALL    劔
      劙劒劒劥劒劒劒劥劒劒劒劥劒劒劒劥劒劒劒劒劒劒劒劥劒劒劒劒劒劒劒劜
      劔  1 劔  --  劔  --  劔  --  劔    NORMAL    劔    NORMAL    劔
      劘劒劒劤劒劒劒劤劒劒劒劤劒劒劒劤劒劒劒劒劒劒劒劤劒劒劒劒劒劒劒劗
        *1丗幚嵺偵偼嬛巭
        *2丗HDTV偱偼 LTD_4thME 偑壜擻偱偁傞偑丄SDTV偵崌傢偣偰 LTD_3rdME 偱
            巊梡偡傞丅乮4M/E帪偼丄WINDOW堐帩偺曽傪桪愭乯


  奺儌乕僪偼埲壓偺捠傝偲側傞丅
  儕僄儞僩儕傪庢偭偰偄側偄 M/E 椶 傪乽侾抜栚乿偲偡傞丅
  側偍乽惂尷偁傝乿偼乽儕僄儞僩儕偼晄壜 (曐徹偱偒側偄)乿偲偄偆堄枴偱偁傞丅

    丒Normal   丗惂尷側偟丅
    丒LTD_4thME丗係抜栚埲崀偺 M/E 偲 FloatingKey丄Additional-PP 偱惂尷偁傝丅
    丒LTD_3rdME丗俁抜栚埲崀偺 M/E 偲 FloatingKey丄Additional-PP 偱惂尷偁傝丅
    丒LTD_All  丗慡偰偺 M/E丄FloatingKey丄Additional-PP 偱惂尷偁傝丅

      LTD_All 偱偼丄僉乕儎乕偱儕僄儞僩儕傪庢傞偙偲偼偱偒側偄丅


    偝傜偵丄拲堄帠崁偑偁傞丅       [MVS:4822]

      3M/E帪偱偡偑丄Multi-Format婎斅偺SD摦嶌帪偵栤戣偑偁傝傑偡丅
      CCR傪庢偭偨偆偊偵僼儖儕僄儞僩儕乕偡傞偨傔偵偼丄TBC_Window_Keep
      偺BIT-SW傪OFF偵偡傞昁梫偑偁傝傑偡丅

      Multi婎斅偱3M/E峔惉偺応崌丄婛偵弌壸偝傟偰偄傞暘偵偮偄偰偼丄
      TBC_Window_Keep偺BIT偑棫偭偰偄傞偼偢側偺偱丄偙傟傪OFF偟偰
      儕僄儞僩儕乕偱偒傞傛偆偵偡傞偐丄偦偺傑傑偵偟偰偍偄偰CCR巊梡帪偵
      俁抜栚偐傜儕僄儞僩儕乕惂尷偑偐偐傞偐丄偺擇戰偵側傞偲巚傢傟傑偡丅
      仸儕僄儞僩儕乕婡擻傪桪愭偡傞偐丄Window堐帩傪桪愭偡傞偐丅


Appendix-3. CPU module 忋偺 Dip Switch SW2 偵傛傞 ME 婎斅悢愝掕 仮c9 捛壛

    仦 ME 峔惉屌掕婡擻

      WELT 側偳偱敪惗偟偰偄傞僔僗僥儉婲摦帪偺 ME 婎斅偺擣幆悢偵
      婲場偡傞儔僀儞棊偪傪媬嵪偡傞偨傔丄僔僗僥儉偺 ME 婎斅悢傪
      帠慜偵屌掕偡傞巇慻傒傪梡堄偡傞丅
      僔僗僥儉偺 ME 婎斅悢偼 CPU module 忋偺 Dip Switch SW2 傪巊偭偰
      愝掕偡傞傕偺偲偡傞丅(DR/DT 嫟捠)

        SW2      DIP SW    bit
        SW2-5  DIP SW bit4   4
        SW2-4  DIP SW bit3   3
        SW2-3  DIP SW bit2   2
        SW2-2  DIP SW bit1   1
        SW2-1  DIP SW bit0   0

      SW2-4 偱廬棃儌乕僪偲 ME 悢屌掕儌乕僪傪愗懼偊傞丅

        摦嶌儌乕僪      bit0
        --------------------
        廬棃儌乕僪       0
        ME 悢屌掕儌乕僪  1

      SW2-2 偲 SW2-3 偱 ME 婎斅悢 1 乣 4 傪昞偡傕偺偲偡傞丅

        ME 婎斅悢  bit2 bit1
        --------------------
            4       1    1
            3       1    0
            2       0    1
            1       0    0
