1 B +8V (ONE END OF POT)

2 C +2V (OTHER END OF POT)

3 NC

4 A ZOOM SPEED (WIPER)

5 D +5V (ZOOM POT CENTER TAP)

6 NC

7 NC

8 NC

9 F VTR RECORD

10 E VTR RECORD

11 H RETURN

12 G RETURN