ADAM POWER SUPPLY FUSE 10/15/2012

	The wires are color coded to for identification,
White/Blue for 2.1v rail
White/Red for +15v rail
Red for 5v rail
White/Orange for -15v rail

There are two 5v rail lines, each are 20A fuses;
The 2.1v fuse is 3A
The +15v fuse is 12A
The -15v fuse is 8A