* The new cards have a smaller package oscillator that fixed the Studer jitter tolerance problem.
* They also have inductors to quiet the power noise near the Cypress chips.
* The power supply was replaced with a linear supply to remove switching noise. The new supply has a heat sink to the board.
* Madi software is version 2.1.1.



