# Configuration file generated by pwmconfig, changes will be lost
INTERVAL=5
DEVPATH=hwmon1=devices/platform/w83627ehf.3232
DEVNAME=hwmon1=w83627dhg
FCTEMPS=hwmon1/device/pwm4=hwmon1/device/temp1_input hwmon1/device/pwm2=hwmon1/device/temp1_input
FCFANS=hwmon1/device/pwm4=hwmon1/device/fan4_input hwmon1/device/pwm2=hwmon1/device/fan2_input
MINTEMP=hwmon1/device/pwm4=20 hwmon1/device/pwm2=20
MAXTEMP=hwmon1/device/pwm4=60 hwmon1/device/pwm2=60
MINSTART=hwmon1/device/pwm4=150 hwmon1/device/pwm2=150
MINSTOP=hwmon1/device/pwm4=0 hwmon1/device/pwm2=0
